(kicad_sch (version 20211123) (generator eeschema)

  (uuid 9538e4ed-27e6-4c37-b989-9859dc0d49e8)

  (paper "A4")

  (lib_symbols
    (symbol "Connector:Conn_01x04_Female" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 5.08 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "Conn_01x04_Female" (id 1) (at 0 -7.62 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "connector" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "Conn_01x04_Female_1_1"
        (arc (start 0 -4.572) (mid -0.508 -5.08) (end 0 -5.588)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 0 -2.032) (mid -0.508 -2.54) (end 0 -3.048)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -5.08)
            (xy -0.508 -5.08)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -2.54)
            (xy -0.508 -2.54)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy -0.508 0)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 2.54)
            (xy -0.508 2.54)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 0 0.508) (mid -0.508 0) (end 0 -0.508)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 0 3.048) (mid -0.508 2.54) (end 0 2.032)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_1" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_2" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_3" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_4" (effects (font (size 1.27 1.27))))
          (number "4" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Connector:Conn_01x08_Female" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 10.16 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "Conn_01x08_Female" (id 1) (at 0 -12.7 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "connector" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "Conn_01x08_Female_1_1"
        (arc (start 0 -9.652) (mid -0.508 -10.16) (end 0 -10.668)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 0 -7.112) (mid -0.508 -7.62) (end 0 -8.128)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 0 -4.572) (mid -0.508 -5.08) (end 0 -5.588)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 0 -2.032) (mid -0.508 -2.54) (end 0 -3.048)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -10.16)
            (xy -0.508 -10.16)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -7.62)
            (xy -0.508 -7.62)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -5.08)
            (xy -0.508 -5.08)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -2.54)
            (xy -0.508 -2.54)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy -0.508 0)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 2.54)
            (xy -0.508 2.54)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 5.08)
            (xy -0.508 5.08)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 7.62)
            (xy -0.508 7.62)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 0 0.508) (mid -0.508 0) (end 0 -0.508)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 0 3.048) (mid -0.508 2.54) (end 0 2.032)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 0 5.588) (mid -0.508 5.08) (end 0 4.572)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (arc (start 0 8.128) (mid -0.508 7.62) (end 0 7.112)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (pin passive line (at -5.08 7.62 0) (length 3.81)
          (name "Pin_1" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "Pin_2" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_3" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_4" (effects (font (size 1.27 1.27))))
          (number "4" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_5" (effects (font (size 1.27 1.27))))
          (number "5" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_6" (effects (font (size 1.27 1.27))))
          (number "6" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 -7.62 0) (length 3.81)
          (name "Pin_7" (effects (font (size 1.27 1.27))))
          (number "7" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 -10.16 0) (length 3.81)
          (name "Pin_8" (effects (font (size 1.27 1.27))))
          (number "8" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Value" "C" (id 1) (at 0.635 -2.54 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (stroke (width 0.508) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (stroke (width 0.508) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Device:Crystal" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Y" (id 0) (at 0 3.81 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "Crystal" (id 1) (at 0 -3.81 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "quartz ceramic resonator oscillator" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Two pin crystal" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Crystal*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "Crystal_0_1"
        (rectangle (start -1.143 2.54) (end 1.143 -2.54)
          (stroke (width 0.3048) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy -1.905 0)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
          )
          (stroke (width 0.508) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.905 -1.27)
            (xy 1.905 1.27)
          )
          (stroke (width 0.508) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 1.905 0)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "Crystal_1_1"
        (pin passive line (at -3.81 0 0) (length 1.27)
          (name "1" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "2" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "R" (id 1) (at 0 0 90)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at -1.778 0 90)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Resistor" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Interface_CAN_LIN:MCP2515-xSO" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -10.16 19.685 0)
        (effects (font (size 1.27 1.27)) (justify right))
      )
      (property "Value" "MCP2515-xSO" (id 1) (at 19.05 20.32 0)
        (effects (font (size 1.27 1.27)) (justify right top))
      )
      (property "Footprint" "Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm" (id 2) (at 0 -22.86 0)
        (effects (font (size 1.27 1.27) italic) hide)
      )
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21801e.pdf" (id 3) (at 2.54 -20.32 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "CAN Controller SPI" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Stand-Alone CAN Controller with SPI Interface, SOIC-18" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "SOIC*7.5x11.6mm*P1.27mm*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "MCP2515-xSO_0_1"
        (rectangle (start -12.7 17.78) (end 12.7 -17.78)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
      )
      (symbol "MCP2515-xSO_1_1"
        (pin output line (at 15.24 12.7 180) (length 2.54)
          (name "TXCAN" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin output line (at 15.24 -5.08 180) (length 2.54)
          (name "~{RX1BF}" (effects (font (size 1.27 1.27))))
          (number "10" (effects (font (size 1.27 1.27))))
        )
        (pin output line (at 15.24 -2.54 180) (length 2.54)
          (name "~{RX0BF}" (effects (font (size 1.27 1.27))))
          (number "11" (effects (font (size 1.27 1.27))))
        )
        (pin output line (at 15.24 0 180) (length 2.54)
          (name "~{INT}" (effects (font (size 1.27 1.27))))
          (number "12" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -15.24 7.62 0) (length 2.54)
          (name "SCK" (effects (font (size 1.27 1.27))))
          (number "13" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -15.24 15.24 0) (length 2.54)
          (name "SI" (effects (font (size 1.27 1.27))))
          (number "14" (effects (font (size 1.27 1.27))))
        )
        (pin output line (at -15.24 12.7 0) (length 2.54)
          (name "SO" (effects (font (size 1.27 1.27))))
          (number "15" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -15.24 10.16 0) (length 2.54)
          (name "~{CS}" (effects (font (size 1.27 1.27))))
          (number "16" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at 15.24 -15.24 180) (length 2.54)
          (name "~{RESET}" (effects (font (size 1.27 1.27))))
          (number "17" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at 0 20.32 270) (length 2.54)
          (name "VDD" (effects (font (size 1.27 1.27))))
          (number "18" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at 15.24 15.24 180) (length 2.54)
          (name "RXCAN" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin output line (at -15.24 -10.16 0) (length 2.54)
          (name "CLKOUT/SOF" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at 15.24 -7.62 180) (length 2.54)
          (name "~{TX0RTS}" (effects (font (size 1.27 1.27))))
          (number "4" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at 15.24 -10.16 180) (length 2.54)
          (name "~{TX1RTS}" (effects (font (size 1.27 1.27))))
          (number "5" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at 15.24 -12.7 180) (length 2.54)
          (name "~{TX2RTS}" (effects (font (size 1.27 1.27))))
          (number "6" (effects (font (size 1.27 1.27))))
        )
        (pin output line (at -15.24 -5.08 0) (length 2.54)
          (name "OSC2" (effects (font (size 1.27 1.27))))
          (number "7" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -15.24 -7.62 0) (length 2.54)
          (name "OSC1" (effects (font (size 1.27 1.27))))
          (number "8" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at 0 -20.32 90) (length 2.54)
          (name "VSS" (effects (font (size 1.27 1.27))))
          (number "9" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Interface_CAN_LIN:TJA1051T" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -10.16 8.89 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Value" "TJA1051T" (id 1) (at 1.27 8.89 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (id 2) (at 0 -12.7 0)
        (effects (font (size 1.27 1.27) italic) hide)
      )
      (property "Datasheet" "http://www.nxp.com/documents/data_sheet/TJA1051.pdf" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "High-Speed CAN Transceiver" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "High-Speed CAN Transceiver, silent mode, SOIC-8" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "TJA1051T_0_1"
        (rectangle (start -10.16 7.62) (end 10.16 -7.62)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
      )
      (symbol "TJA1051T_1_1"
        (pin input line (at -12.7 5.08 0) (length 2.54)
          (name "TXD" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at 0 -10.16 90) (length 2.54)
          (name "GND" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at 0 10.16 270) (length 2.54)
          (name "VCC" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
        (pin output line (at -12.7 2.54 0) (length 2.54)
          (name "RXD" (effects (font (size 1.27 1.27))))
          (number "4" (effects (font (size 1.27 1.27))))
        )
        (pin no_connect line (at -12.7 -2.54 0) (length 2.54) hide
          (name "n.c." (effects (font (size 1.27 1.27))))
          (number "5" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
          (name "CANL" (effects (font (size 1.27 1.27))))
          (number "6" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 12.7 2.54 180) (length 2.54)
          (name "CANH" (effects (font (size 1.27 1.27))))
          (number "7" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -12.7 -5.08 0) (length 2.54)
          (name "S" (effects (font (size 1.27 1.27))))
          (number "8" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Jumper:Jumper_2_Open" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (id 0) (at 0 2.794 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "Jumper_2_Open" (id 1) (at 0 -2.286 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "Jumper SPST" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Jumper, 2-pole, open" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Jumper* TestPoint*2Pads* TestPoint*Bridge*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "Jumper_2_Open_0_0"
        (circle (center -2.032 0) (radius 0.508)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "Jumper_2_Open_0_1"
        (arc (start 1.524 1.27) (mid 0 1.778) (end -1.524 1.27)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "Jumper_2_Open_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "A" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "B" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "MCU_Microchip_ATmega:ATmega4809-A" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -12.7 34.29 0)
        (effects (font (size 1.27 1.27)) (justify left bottom))
      )
      (property "Value" "ATmega4809-A" (id 1) (at 2.54 -34.29 0)
        (effects (font (size 1.27 1.27)) (justify left top))
      )
      (property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27) italic) hide)
      )
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40002016A.pdf" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "AVR 8bit Microcontroller MegaAVR" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "20MHz, 48kB Flash, 6kB SRAM, 256B EEPROM, TQFP-48" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "ATmega4809-A_0_1"
        (rectangle (start -12.7 -33.02) (end 12.7 33.02)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
      )
      (symbol "ATmega4809-A_1_1"
        (pin bidirectional line (at 15.24 17.78 180) (length 2.54)
          (name "PA5" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
          (name "PC0" (effects (font (size 1.27 1.27))))
          (number "10" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 -12.7 180) (length 2.54)
          (name "PC1" (effects (font (size 1.27 1.27))))
          (number "11" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 -15.24 180) (length 2.54)
          (name "PC2" (effects (font (size 1.27 1.27))))
          (number "12" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 -17.78 180) (length 2.54)
          (name "PC3" (effects (font (size 1.27 1.27))))
          (number "13" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at 0 35.56 270) (length 2.54)
          (name "VCC" (effects (font (size 1.27 1.27))))
          (number "14" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at 0 -35.56 90) (length 2.54)
          (name "GND" (effects (font (size 1.27 1.27))))
          (number "15" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 -20.32 180) (length 2.54)
          (name "PC4" (effects (font (size 1.27 1.27))))
          (number "16" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 -22.86 180) (length 2.54)
          (name "PC5" (effects (font (size 1.27 1.27))))
          (number "17" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 -25.4 180) (length 2.54)
          (name "PC6" (effects (font (size 1.27 1.27))))
          (number "18" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 -27.94 180) (length 2.54)
          (name "PC7" (effects (font (size 1.27 1.27))))
          (number "19" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
          (name "PA6" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 -10.16 0) (length 2.54)
          (name "PD0" (effects (font (size 1.27 1.27))))
          (number "20" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 -12.7 0) (length 2.54)
          (name "PD1" (effects (font (size 1.27 1.27))))
          (number "21" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 -15.24 0) (length 2.54)
          (name "PD2" (effects (font (size 1.27 1.27))))
          (number "22" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 -17.78 0) (length 2.54)
          (name "PD3" (effects (font (size 1.27 1.27))))
          (number "23" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 -20.32 0) (length 2.54)
          (name "PD4" (effects (font (size 1.27 1.27))))
          (number "24" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 -22.86 0) (length 2.54)
          (name "PD5" (effects (font (size 1.27 1.27))))
          (number "25" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 -25.4 0) (length 2.54)
          (name "PD6" (effects (font (size 1.27 1.27))))
          (number "26" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 -27.94 0) (length 2.54)
          (name "PD7" (effects (font (size 1.27 1.27))))
          (number "27" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at 2.54 35.56 270) (length 2.54)
          (name "AVCC" (effects (font (size 1.27 1.27))))
          (number "28" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -35.56 90) (length 2.54) hide
          (name "GND" (effects (font (size 1.27 1.27))))
          (number "29" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 12.7 180) (length 2.54)
          (name "PA7" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 5.08 0) (length 2.54)
          (name "PE0" (effects (font (size 1.27 1.27))))
          (number "30" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 2.54 0) (length 2.54)
          (name "PE1" (effects (font (size 1.27 1.27))))
          (number "31" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 0 0) (length 2.54)
          (name "PE2" (effects (font (size 1.27 1.27))))
          (number "32" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 -2.54 0) (length 2.54)
          (name "PE3" (effects (font (size 1.27 1.27))))
          (number "33" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 25.4 0) (length 2.54)
          (name "PF0" (effects (font (size 1.27 1.27))))
          (number "34" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 22.86 0) (length 2.54)
          (name "PF1" (effects (font (size 1.27 1.27))))
          (number "35" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 20.32 0) (length 2.54)
          (name "PF2" (effects (font (size 1.27 1.27))))
          (number "36" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 17.78 0) (length 2.54)
          (name "PF3" (effects (font (size 1.27 1.27))))
          (number "37" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 15.24 0) (length 2.54)
          (name "PF4" (effects (font (size 1.27 1.27))))
          (number "38" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 12.7 0) (length 2.54)
          (name "PF5" (effects (font (size 1.27 1.27))))
          (number "39" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
          (name "PB0" (effects (font (size 1.27 1.27))))
          (number "4" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 10.16 0) (length 2.54)
          (name "PF6/~{RESET}" (effects (font (size 1.27 1.27))))
          (number "40" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at -15.24 30.48 0) (length 2.54)
          (name "UPDI" (effects (font (size 1.27 1.27))))
          (number "41" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 35.56 270) (length 2.54) hide
          (name "VCC" (effects (font (size 1.27 1.27))))
          (number "42" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -35.56 90) (length 2.54) hide
          (name "GND" (effects (font (size 1.27 1.27))))
          (number "43" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 30.48 180) (length 2.54)
          (name "PA0" (effects (font (size 1.27 1.27))))
          (number "44" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 27.94 180) (length 2.54)
          (name "PA1" (effects (font (size 1.27 1.27))))
          (number "45" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 25.4 180) (length 2.54)
          (name "PA2" (effects (font (size 1.27 1.27))))
          (number "46" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 22.86 180) (length 2.54)
          (name "PA3" (effects (font (size 1.27 1.27))))
          (number "47" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 20.32 180) (length 2.54)
          (name "PA4" (effects (font (size 1.27 1.27))))
          (number "48" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
          (name "PB1" (effects (font (size 1.27 1.27))))
          (number "5" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
          (name "PB2" (effects (font (size 1.27 1.27))))
          (number "6" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 0 180) (length 2.54)
          (name "PB3" (effects (font (size 1.27 1.27))))
          (number "7" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
          (name "PB4" (effects (font (size 1.27 1.27))))
          (number "8" (effects (font (size 1.27 1.27))))
        )
        (pin bidirectional line (at 15.24 -5.08 180) (length 2.54)
          (name "PB5" (effects (font (size 1.27 1.27))))
          (number "9" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Regulator_Linear:MCP1703A-5002_SOT23" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -3.81 3.175 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "MCP1703A-5002_SOT23" (id 1) (at 0 3.175 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 0 5.08 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf" (id 3) (at 0 -1.27 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "REGULATOR LDO" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Low Quiescent Current LDO Regulator, 5.0V, 250mA, Vin<=16V, SOT-23" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "MCP1703A-5002_SOT23_0_1"
        (rectangle (start -5.08 -5.08) (end 5.08 1.905)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
      )
      (symbol "MCP1703A-5002_SOT23_1_1"
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin power_out line (at 7.62 0 180) (length 2.54)
          (name "VO" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at -7.62 0 0) (length 2.54)
          (name "VI" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Value" "+5V" (id 1) (at 0 3.556 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "power:GNDREF" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Value" "GNDREF" (id 1) (at 0 -3.81 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Power symbol creates a global label with name \"GNDREF\" , reference supply ground" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "GNDREF_0_1"
        (polyline
          (pts
            (xy -0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.127 -2.54)
            (xy 0.127 -2.54)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -1.27)
            (xy 0 0)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy -1.27 -1.27)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "GNDREF_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GNDREF" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
      )
    )
  )

  (junction (at 177.8 78.74) (diameter 0) (color 0 0 0 0)
    (uuid 0228b435-2206-444b-b9ab-79103ff4d808)
  )
  (junction (at 177.8 147.32) (diameter 0) (color 0 0 0 0)
    (uuid 0da4f391-9874-4685-8800-9524303c153e)
  )
  (junction (at 48.26 63.5) (diameter 0) (color 0 0 0 0)
    (uuid 24421ba2-f6c8-428f-aac0-7e5ffea4e133)
  )
  (junction (at 133.35 86.36) (diameter 0) (color 0 0 0 0)
    (uuid 25c8f0d8-f09e-41d0-bfd7-a6cf8f51af92)
  )
  (junction (at 133.35 83.82) (diameter 0) (color 0 0 0 0)
    (uuid 42ebe32d-b2c7-47dc-86c0-d5f770977a21)
  )
  (junction (at 44.45 48.26) (diameter 0) (color 0 0 0 0)
    (uuid 45b3c739-69dd-4e8b-b93d-58fdc3828bf4)
  )
  (junction (at 128.27 134.62) (diameter 0) (color 0 0 0 0)
    (uuid 612d0e45-7497-483c-8e3a-ede96888ac5e)
  )
  (junction (at 128.27 147.32) (diameter 0) (color 0 0 0 0)
    (uuid 61bd52d5-d680-4281-a0a6-1299fe085462)
  )
  (junction (at 138.43 86.36) (diameter 0) (color 0 0 0 0)
    (uuid 75918951-9205-46b0-8175-c2534df75528)
  )
  (junction (at 177.8 53.34) (diameter 0) (color 0 0 0 0)
    (uuid 78a0f37a-86af-4294-920e-127685718102)
  )
  (junction (at 85.09 147.32) (diameter 0) (color 0 0 0 0)
    (uuid 7b98ebd8-cf86-4a46-8603-06f8e0517b2d)
  )
  (junction (at 128.27 144.78) (diameter 0) (color 0 0 0 0)
    (uuid 81b1a1fe-4122-45f5-a4ae-1357a3162812)
  )
  (junction (at 133.35 53.34) (diameter 0) (color 0 0 0 0)
    (uuid 88b37e8b-d98a-4e5d-81ec-b6e67b18ded5)
  )
  (junction (at 44.45 45.72) (diameter 0) (color 0 0 0 0)
    (uuid 9c09e03c-c22a-44f6-b480-f2d3e22ea245)
  )
  (junction (at 48.26 83.82) (diameter 0) (color 0 0 0 0)
    (uuid ac0c8e91-d596-420a-9d9b-488e32d73738)
  )
  (junction (at 74.93 43.18) (diameter 0) (color 0 0 0 0)
    (uuid d342926e-ab33-4291-a89e-62a463cb9800)
  )
  (junction (at 138.43 147.32) (diameter 0) (color 0 0 0 0)
    (uuid f55371d2-3db1-4cba-87ff-cf6ae6c7f42a)
  )
  (junction (at 67.31 40.64) (diameter 0) (color 0 0 0 0)
    (uuid feb390f5-780f-46bd-bf7e-34105cb72e0a)
  )

  (wire (pts (xy 48.26 83.82) (xy 48.26 147.32))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 007dbeaf-917e-4a9f-b3a4-ce947d107501)
  )
  (wire (pts (xy 138.43 147.32) (xy 177.8 147.32))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 06c5e84e-b370-44f3-86da-6cefda34cf80)
  )
  (wire (pts (xy 156.21 86.36) (xy 138.43 86.36))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 0799e38d-4fc2-4e88-afee-ab6769cbe73d)
  )
  (wire (pts (xy 138.43 95.25) (xy 138.43 147.32))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 0ce83393-6fb7-4d87-b607-25c1c509e373)
  )
  (wire (pts (xy 97.79 99.06) (xy 97.79 125.73))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 0d6f0839-7210-4f59-b623-c5f1afbf9614)
  )
  (wire (pts (xy 87.63 124.46) (xy 85.09 124.46))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 0e838392-bb0a-408a-9aad-59bcfc3cfb02)
  )
  (wire (pts (xy 133.35 53.34) (xy 133.35 83.82))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 120eae6e-d2f6-4d9a-8014-666c79fa1758)
  )
  (wire (pts (xy 162.56 105.41) (xy 156.21 105.41))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 13292a60-2c49-47b7-9468-ebf1a36b7873)
  )
  (wire (pts (xy 222.25 53.34) (xy 222.25 97.79))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 15b513d6-12bd-4f61-9bf6-23840bb549e5)
  )
  (wire (pts (xy 95.25 99.06) (xy 95.25 125.73))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 17aa414a-03b0-4d0e-873d-63d73ab6d574)
  )
  (wire (pts (xy 194.31 78.74) (xy 199.39 78.74))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 187b1562-c7f2-4a50-9551-0d5ec51704bb)
  )
  (wire (pts (xy 113.03 107.95) (xy 162.56 107.95))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 190eb1fb-24f2-4efb-aee5-02321e3be447)
  )
  (wire (pts (xy 67.31 24.13) (xy 74.93 24.13))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 1fccfb79-21a3-4510-bc90-3b48f7cfdbce)
  )
  (wire (pts (xy 128.27 144.78) (xy 128.27 147.32))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 22845a61-3701-4be2-a628-3e70dd387b44)
  )
  (wire (pts (xy 48.26 147.32) (xy 85.09 147.32))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 24a9118d-cb2b-4cb0-af96-8935ddca583c)
  )
  (wire (pts (xy 193.04 102.87) (xy 209.55 102.87))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 263af5f9-896d-4f09-96e3-58c64c70e1cb)
  )
  (wire (pts (xy 128.27 137.16) (xy 128.27 134.62))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 27944d43-cfdb-48b0-ab98-286b16d4115b)
  )
  (wire (pts (xy 115.57 102.87) (xy 162.56 102.87))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 2941814c-06bd-4877-989a-6d36fe7ef69b)
  )
  (wire (pts (xy 177.8 78.74) (xy 186.69 78.74))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 295670b9-0c07-4238-8f56-20642969e240)
  )
  (wire (pts (xy 44.45 40.64) (xy 67.31 40.64))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 2af99217-2ba5-478e-8f35-ea4eb5d8dae5)
  )
  (wire (pts (xy 44.45 45.72) (xy 48.26 45.72))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 2cdc59dd-1a7b-4afd-896b-6dd1d45af6c5)
  )
  (wire (pts (xy 110.49 99.06) (xy 110.49 120.65))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 2e1e3699-c79c-4ed7-bdf0-60aa34df84fd)
  )
  (wire (pts (xy 26.67 53.34) (xy 26.67 45.72))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 3018567d-4753-4b2f-9f86-8cdd84859300)
  )
  (wire (pts (xy 177.8 78.74) (xy 177.8 95.25))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 3380a877-cd4b-4b6d-ac17-d63674e32a7a)
  )
  (wire (pts (xy 67.31 36.83) (xy 67.31 40.64))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 3394b2b1-594a-42ad-ad3e-94ca3555c51c)
  )
  (wire (pts (xy 115.57 99.06) (xy 115.57 102.87))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 35e89e90-557b-419d-bb99-a89abbd598f8)
  )
  (wire (pts (xy 26.67 45.72) (xy 44.45 45.72))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 3984d725-0604-4580-8447-a030e380a70d)
  )
  (wire (pts (xy 100.33 99.06) (xy 100.33 125.73))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 3c4c0cf3-189d-475a-99d1-b7e4a2b31098)
  )
  (wire (pts (xy 67.31 40.64) (xy 256.54 40.64))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 3cff355f-4467-442f-af03-c7a4b9c1492d)
  )
  (wire (pts (xy 29.21 48.26) (xy 44.45 48.26))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 4a918663-0357-498d-ac19-009bb4a4714e)
  )
  (wire (pts (xy 44.45 48.26) (xy 44.45 53.34))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 4b356248-8800-46a4-8e12-1cd1f4f5993d)
  )
  (wire (pts (xy 68.58 53.34) (xy 133.35 53.34))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 4fef87af-a2b0-47ea-9970-39577b5d860b)
  )
  (wire (pts (xy 44.45 53.34) (xy 53.34 53.34))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 520984f5-7893-4082-bcf9-a031ad16a0db)
  )
  (wire (pts (xy 74.93 24.13) (xy 74.93 27.94))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 54b51d31-2349-4972-8c28-b2ae1a316391)
  )
  (wire (pts (xy 118.11 99.06) (xy 118.11 100.33))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 562ab560-81ce-47ea-b7d2-896ce91ff717)
  )
  (wire (pts (xy 256.54 40.64) (xy 256.54 110.49))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 5abaf27b-4049-4867-99b4-20f587aff838)
  )
  (wire (pts (xy 177.8 53.34) (xy 177.8 78.74))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 5b1a7623-6622-4e16-b769-fb4202b3b4ea)
  )
  (wire (pts (xy 199.39 120.65) (xy 193.04 120.65))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 658ca670-b095-48fb-ba6b-a75e296e209c)
  )
  (wire (pts (xy 74.93 35.56) (xy 74.93 43.18))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 6625711a-832e-4e8d-9de4-7d91e05c5893)
  )
  (wire (pts (xy 29.21 39.37) (xy 29.21 48.26))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 665d705a-aa1d-46ab-8d69-540cdf1ac1f7)
  )
  (wire (pts (xy 114.3 134.62) (xy 118.11 134.62))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 6bd51e34-8267-4f86-bcce-2c7de1c0f372)
  )
  (wire (pts (xy 234.95 110.49) (xy 256.54 110.49))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 6c2ef669-8701-4a7e-a9fc-bc4bdbe4c922)
  )
  (wire (pts (xy 114.3 144.78) (xy 128.27 144.78))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 6db80c70-0cd1-4b05-96b3-b978167a2cc8)
  )
  (wire (pts (xy 133.35 86.36) (xy 133.35 83.82))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 6f296356-db92-4eda-be34-a000ff7c335d)
  )
  (wire (pts (xy 234.95 105.41) (xy 254 105.41))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 7e5e7021-b1cd-4e41-8140-fda1fc5b4b0b)
  )
  (wire (pts (xy 128.27 147.32) (xy 138.43 147.32))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 8122812f-97dd-4aea-a57d-db3c7cc681d1)
  )
  (wire (pts (xy 113.03 99.06) (xy 113.03 107.95))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 84cb22d0-d583-4c84-b2a2-918aaaa9d538)
  )
  (wire (pts (xy 105.41 99.06) (xy 105.41 125.73))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 866c3861-ee39-40b6-a8ac-61c20495fd6e)
  )
  (wire (pts (xy 196.85 100.33) (xy 196.85 105.41))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 88448c25-3fc9-4e98-a9da-7656e88cada1)
  )
  (wire (pts (xy 133.35 86.36) (xy 138.43 86.36))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 8a7e734c-d935-4549-943b-c8fab9438291)
  )
  (wire (pts (xy 196.85 105.41) (xy 209.55 105.41))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 8ced3a31-1359-4152-808d-8b5a468b2a9e)
  )
  (wire (pts (xy 177.8 53.34) (xy 222.25 53.34))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 9c255290-f1be-486c-97c3-4917c1216fce)
  )
  (wire (pts (xy 177.8 135.89) (xy 177.8 147.32))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 9cc297a4-ffc3-4ed2-b1a1-4feae5235fa7)
  )
  (wire (pts (xy 74.93 43.18) (xy 254 43.18))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 9fb67d89-c845-475f-941e-35ee6347b307)
  )
  (wire (pts (xy 48.26 83.82) (xy 62.23 83.82))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid a6ffade5-89d5-478f-826b-2051927e247e)
  )
  (wire (pts (xy 177.8 147.32) (xy 222.25 147.32))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid a92f1016-ab32-4c5d-97b8-e82147da8f51)
  )
  (wire (pts (xy 48.26 63.5) (xy 60.96 63.5))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid afe6acf0-6998-42eb-8428-627ecbdc0004)
  )
  (wire (pts (xy 48.26 45.72) (xy 48.26 63.5))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid bb3ada41-c26f-4236-b74e-16450f55c575)
  )
  (wire (pts (xy 67.31 26.67) (xy 67.31 24.13))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid bbd519e1-7064-48e2-a43f-cf059210d11f)
  )
  (wire (pts (xy 128.27 134.62) (xy 125.73 134.62))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid bdff4025-f63a-4124-bad4-d6e0589a28af)
  )
  (wire (pts (xy 114.3 137.16) (xy 114.3 134.62))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid be9f996f-bf82-4348-a7c7-bdc706bc16b8)
  )
  (wire (pts (xy 128.27 99.06) (xy 128.27 134.62))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid bfd2d2bd-2ca2-4da3-b7bd-5e442242c9a3)
  )
  (wire (pts (xy 254 43.18) (xy 254 105.41))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid c48d63e0-832e-4d2f-b341-bb5cb392f885)
  )
  (wire (pts (xy 199.39 78.74) (xy 199.39 120.65))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid c59b0e0c-401b-40b5-95c5-4b190c5e6579)
  )
  (wire (pts (xy 222.25 118.11) (xy 222.25 147.32))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid c6862845-285e-47cb-b11a-fde25f379e8b)
  )
  (wire (pts (xy 87.63 125.73) (xy 87.63 124.46))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid c842be6a-877f-407f-b178-2425797cd309)
  )
  (wire (pts (xy 110.49 120.65) (xy 162.56 120.65))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid c8b41c77-dba6-4fa6-bb77-e6de7f86e53c)
  )
  (wire (pts (xy 118.11 100.33) (xy 162.56 100.33))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid cf210172-6d8f-4405-82e8-f991357fa105)
  )
  (wire (pts (xy 133.35 53.34) (xy 177.8 53.34))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid d2c43a14-1e0c-4947-a6d1-2f5c3adcf510)
  )
  (wire (pts (xy 44.45 43.18) (xy 74.93 43.18))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid dbc3ccca-82de-4839-a12e-ceaeacfbd8e9)
  )
  (wire (pts (xy 48.26 63.5) (xy 48.26 83.82))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid e1f0182b-61ba-4040-b7d9-35aa878312aa)
  )
  (wire (pts (xy 85.09 147.32) (xy 128.27 147.32))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid e40eff05-1192-431f-9fe7-c855ef15c3c9)
  )
  (wire (pts (xy 156.21 86.36) (xy 156.21 105.41))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid e7a952b5-8b07-4111-b97b-edfe92082f13)
  )
  (wire (pts (xy 85.09 124.46) (xy 85.09 147.32))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid e82214b7-1ba3-460a-9922-39406a021fcd)
  )
  (wire (pts (xy 138.43 86.36) (xy 138.43 87.63))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid ef63838e-669e-42e6-a536-f75949d5c967)
  )
  (wire (pts (xy 102.87 99.06) (xy 102.87 125.73))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid f5f3b6b6-54c4-490f-8236-d7513b1332df)
  )
  (wire (pts (xy 92.71 99.06) (xy 92.71 125.73))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid f78aa980-926b-4b0f-94c3-31a6beb7e5f0)
  )
  (wire (pts (xy 193.04 100.33) (xy 196.85 100.33))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid fb61fca8-c296-4f28-9652-e8a0e9108b6b)
  )
  (wire (pts (xy 60.96 60.96) (xy 60.96 63.5))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid fc9b2a04-fcf3-412f-b61a-caccdc02781a)
  )

  (symbol (lib_id "Jumper:Jumper_2_Open") (at 67.31 31.75 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 0ddffb29-819f-4fb1-8ac1-f59fa3272ba3)
    (property "Reference" "JP1" (id 0) (at 68.58 30.4799 90)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "Jumper_2_Open" (id 1) (at 68.58 33.0199 90)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "" (id 2) (at 67.31 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 67.31 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid b69068bb-bb06-4b8d-b2a3-cec673a6145f))
    (pin "2" (uuid da85e218-28f5-4e04-9ae0-77a4ed9bdc04))
  )

  (symbol (lib_id "Connector:Conn_01x04_Female") (at 39.37 45.72 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 2c236797-4e84-4743-80c6-9d38d6188d4c)
    (property "Reference" "J1" (id 0) (at 40.005 35.56 0))
    (property "Value" "Conn_01x04_Female" (id 1) (at 40.005 38.1 0))
    (property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-4-3.5-H_1x04_P3.50mm_Horizontal" (id 2) (at 39.37 45.72 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 39.37 45.72 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 938ba571-7ebe-4d63-bdda-485a4f959fbd))
    (pin "2" (uuid 52b2fe05-2765-440b-ad1a-07ce20eec8e1))
    (pin "3" (uuid 693bd32a-f43e-4503-9d2a-5719166ccddf))
    (pin "4" (uuid fa0fd85b-5610-42fb-9c7b-77905ee396b1))
  )

  (symbol (lib_id "Device:C") (at 138.43 91.44 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 36540234-f263-4775-a9eb-82bf31b6d3b0)
    (property "Reference" "C3" (id 0) (at 142.24 90.1699 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "" (id 1) (at 142.24 92.7099 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 139.3952 95.25 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 138.43 91.44 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid dda9299b-9c5a-4b08-b659-4d46c4154344))
    (pin "2" (uuid cde436aa-9e10-42a7-a055-cbd9c7233469))
  )

  (symbol (lib_id "Interface_CAN_LIN:MCP2515-xSO") (at 177.8 115.57 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 55870dc1-a751-4fb1-a7eb-fe844b64659b)
    (property "Reference" "U1" (id 0) (at 179.8194 92.71 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MCP2515-xSO" (id 1) (at 179.8194 95.25 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 177.8 138.43 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21801e.pdf" (id 3) (at 180.34 135.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid ec1c193f-86ec-48fc-a26b-de8201d681ac))
    (pin "10" (uuid 077985bd-c8a6-43b8-af30-1141a8334306))
    (pin "11" (uuid 3c3e78d8-62d7-4020-ae7c-c489234b27d5))
    (pin "12" (uuid 9caefee8-6dcd-4815-b6e5-c75999fb9c90))
    (pin "13" (uuid 977371ef-232c-40b3-8805-7fed7909b206))
    (pin "14" (uuid e3877396-3ff6-4b1d-9715-0d1a70961579))
    (pin "15" (uuid f094eb5d-05c7-4c16-84d0-9d4665317bfb))
    (pin "16" (uuid 4ff71e44-dddb-450e-9f6f-fe3947968fd4))
    (pin "17" (uuid 138f5600-7fba-4219-9f21-9ce4066a1d82))
    (pin "18" (uuid b5691874-e380-4013-b466-13948504ae2f))
    (pin "2" (uuid 5b86cb50-e2ef-475e-93e3-77fea6b5a690))
    (pin "3" (uuid 7167e0fb-15b0-446d-969c-ecf63e50097d))
    (pin "4" (uuid c25b90aa-c787-46a1-8b80-e5b9fd45039a))
    (pin "5" (uuid 1cd08355-701e-4fba-886f-d48517dcccf5))
    (pin "6" (uuid 2f8dfa45-14b0-4de4-b3b0-e7b73da81a0a))
    (pin "7" (uuid 84282cc7-416d-48c2-ae9f-c0149b35065e))
    (pin "8" (uuid eb79b938-dc23-4503-beb0-3634b653c9e4))
    (pin "9" (uuid c2f8c49f-d49f-49e2-940a-a7b9765ffdf0))
  )

  (symbol (lib_id "Device:R") (at 74.93 31.75 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 58697035-c2a5-4a72-aa6c-0845690bbd5f)
    (property "Reference" "R2" (id 0) (at 77.47 30.4799 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "120" (id 1) (at 77.47 33.0199 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "" (id 2) (at 76.708 31.75 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 74.93 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid b3ef4181-26bd-42ac-8711-a6914ca5f6b0))
    (pin "2" (uuid 00c7f158-18a1-4d5d-8258-3a26fd0c9e5f))
  )

  (symbol (lib_id "power:GNDREF") (at 26.67 53.34 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 6117d579-0678-4c3b-8682-2fe4ddc7a0e7)
    (property "Reference" "#PWR0101" (id 0) (at 26.67 59.69 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Value" "GNDREF" (id 1) (at 26.67 58.42 0))
    (property "Footprint" "" (id 2) (at 26.67 53.34 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 26.67 53.34 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 536fa0ea-21fb-49cd-9a0f-449ea9ab9637))
  )

  (symbol (lib_id "Device:C") (at 128.27 140.97 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 68e9e548-d824-4d92-b10b-c055a20dcada)
    (property "Reference" "C2" (id 0) (at 132.08 139.6999 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "14 pF" (id 1) (at 132.08 142.2399 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "" (id 2) (at 127.3048 137.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 128.27 140.97 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 9eca6f5a-3887-42f3-8c7e-db84e21b4025))
    (pin "2" (uuid 05437f7d-dc7b-4391-aa33-2b9d5b15a0fa))
  )

  (symbol (lib_id "Connector:Conn_01x08_Female") (at 97.79 130.81 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 6b0bd125-8e7d-4e87-97f5-0d4d53faa173)
    (property "Reference" "J2" (id 0) (at 96.52 133.35 90))
    (property "Value" "" (id 1) (at 96.52 135.89 90))
    (property "Footprint" "" (id 2) (at 97.79 130.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 97.79 130.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid dd99ad7e-bdde-4e23-9c38-09719daa5f49))
    (pin "2" (uuid 0ce01842-89f2-423b-8f97-b39044f9ab51))
    (pin "3" (uuid 871c14db-0529-42ab-9d3f-05bba17dfc76))
    (pin "4" (uuid c7b7168e-279d-49ef-902c-f549d2ee2ac1))
    (pin "5" (uuid ba410a01-d7aa-4128-abd0-b5ba9f6b5f46))
    (pin "6" (uuid 08d75b80-46f2-48b7-af19-167e729deb89))
    (pin "7" (uuid 6bc92358-f3a5-48e4-afb6-78839719d659))
    (pin "8" (uuid f56dcb14-12b0-4a9e-8702-800fc866ce43))
  )

  (symbol (lib_id "Regulator_Linear:MCP1703A-5002_SOT23") (at 60.96 53.34 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 70b5de83-b371-4d8a-b6ce-c6eae87736b1)
    (property "Reference" "U3" (id 0) (at 60.96 45.72 0))
    (property "Value" "MCP1703A-5002_SOT23" (id 1) (at 60.96 48.26 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 60.96 48.26 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf" (id 3) (at 60.96 54.61 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid ff985e12-1ba2-49a0-925f-43b9f18cf7f2))
    (pin "2" (uuid 9dc0483a-8625-4de5-93c1-815690c8ddf4))
    (pin "3" (uuid 2c685221-6902-4618-ac8d-0a0f2275c45c))
  )

  (symbol (lib_id "MCU_Microchip_ATmega:ATmega4809-A") (at 97.79 83.82 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 7308e13a-4809-4e8e-af65-9905819aa376)
    (property "Reference" "U4" (id 0) (at 55.88 77.2412 90))
    (property "Value" "" (id 1) (at 55.88 79.7812 90))
    (property "Footprint" "" (id 2) (at 97.79 83.82 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40002016A.pdf" (id 3) (at 97.79 83.82 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 9e5b0177-ea58-4f76-8b57-ff1c6e52d9df))
    (pin "10" (uuid e8cb6cb3-dd2b-4328-8592-132e369ebb71))
    (pin "11" (uuid f630bdcd-b048-45d2-91a0-928349b89dad))
    (pin "12" (uuid c374668c-56af-42dd-a650-35352e96de63))
    (pin "13" (uuid 08d1dac8-0d6e-4029-9a06-c8863d7fbd51))
    (pin "14" (uuid 40962e92-90b6-487d-b0dc-0a6c42b5ebc2))
    (pin "15" (uuid 25b39db8-8576-4473-b331-b912323e85f4))
    (pin "16" (uuid ffde4898-4c0e-4c24-bd8c-aadcd7279172))
    (pin "17" (uuid 5aa0e472-160b-49ac-864f-0fa7cd9cf9b0))
    (pin "18" (uuid 086ab04d-4086-427c-992f-819b91a9021d))
    (pin "19" (uuid 59246647-4e57-4b5f-9f1e-b0cc1fb90bb2))
    (pin "2" (uuid 51bdd1cb-8a01-4b1c-940a-3ff4dd1de87c))
    (pin "20" (uuid 6025c071-1487-4c03-a645-f67437519813))
    (pin "21" (uuid b79d8d99-88b5-4d84-a010-b6d768d67ec8))
    (pin "22" (uuid a2c0fc07-9ed2-42e8-8fef-f02fce3412ee))
    (pin "23" (uuid 0d678ff1-21aa-4e6f-ae06-abf24406f3c8))
    (pin "24" (uuid e7c8f673-e523-47ce-91b8-92cf1c7605ce))
    (pin "25" (uuid eb06cbed-9a37-40e7-bc33-37acd0ee650a))
    (pin "26" (uuid 172b515f-13aa-42a2-b6ac-db67c2e524e7))
    (pin "27" (uuid a5c35670-98af-44c6-a3f4-bbad7ffecfd3))
    (pin "28" (uuid 5bd90e77-727e-49e2-881e-09f4ce3768d4))
    (pin "29" (uuid af7ccd5a-4c05-4a49-a412-ca568e4c81d2))
    (pin "3" (uuid 911557e5-adec-4d13-9794-a18b325eb4ea))
    (pin "30" (uuid d40ed1bf-6a69-492a-acf3-f71f1c7a81f2))
    (pin "31" (uuid 67320774-1745-4c89-bec7-2213f7bb7ecc))
    (pin "32" (uuid cab0d0a9-e089-4f0b-8483-22b4e0addcae))
    (pin "33" (uuid 3c5840eb-164e-426c-ab78-faa89624b9dc))
    (pin "34" (uuid 43b7aab0-ec9b-4c58-bfa1-8dda8fccb53f))
    (pin "35" (uuid 5968c877-7376-4e25-b8db-5e755d570d06))
    (pin "36" (uuid 1cd85cce-d94a-4a92-8af2-23d3a2b66793))
    (pin "37" (uuid a26bc030-7d8a-4b19-aa84-9206cc0de2b0))
    (pin "38" (uuid d66c8b0e-b6b3-43ea-8c6d-9724edcc57d6))
    (pin "39" (uuid 3d19e22b-2666-4e7d-825d-37a04ed07fa1))
    (pin "4" (uuid 054f8e07-0141-451f-a3c4-ea786b83b680))
    (pin "40" (uuid ed6caead-58a0-4a37-97cf-621d3ffb0ca4))
    (pin "41" (uuid 62af6e3c-7d06-438a-b62f-014ae3262ea1))
    (pin "42" (uuid afc1392c-4488-4251-8167-de520abba754))
    (pin "43" (uuid 248d15cd-dd0c-425d-94cb-b44ccf865457))
    (pin "44" (uuid 42688fc6-3e24-4a56-9963-828da46dcdfb))
    (pin "45" (uuid c546008e-7661-419e-94b3-0bbb9fd14ec8))
    (pin "46" (uuid a6460cc6-b11c-4dff-a0ea-9de680e68ca8))
    (pin "47" (uuid 3aec5e23-e675-4bcf-9a9e-48cb59d51927))
    (pin "48" (uuid 01657d30-6f8e-4bbd-a3dd-6a0742c69aca))
    (pin "5" (uuid 72729c20-0465-4f8c-be80-3c22bb337ef7))
    (pin "6" (uuid a5fcd820-f4f0-487d-8e2f-6defe7618982))
    (pin "7" (uuid bf67f245-1714-4d39-b76d-53f1523ab5f8))
    (pin "8" (uuid ccd45da3-3d73-496d-8f2e-5edf69377f63))
    (pin "9" (uuid 0a83f85d-78ad-480a-a5ba-773caced8f09))
  )

  (symbol (lib_id "Device:R") (at 190.5 78.74 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 76ee4584-81e2-4930-acce-1ecd238cf151)
    (property "Reference" "R1" (id 0) (at 190.5 72.39 90))
    (property "Value" "10K" (id 1) (at 190.5 74.93 90))
    (property "Footprint" "" (id 2) (at 190.5 80.518 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 190.5 78.74 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid aa3624e4-78e8-49e2-a323-8e316bcb410b))
    (pin "2" (uuid 6360dc87-de30-4fa1-bcaa-915d4b4ad54c))
  )

  (symbol (lib_id "Device:Crystal") (at 121.92 134.62 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid a9ccf595-ea22-4b8c-914d-3ab6dbf2ada1)
    (property "Reference" "Y1" (id 0) (at 121.92 127 0))
    (property "Value" "" (id 1) (at 121.92 129.54 0))
    (property "Footprint" "" (id 2) (at 121.92 134.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 121.92 134.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid cb888192-401d-4273-96a9-cb25366e59cc))
    (pin "2" (uuid cf17fd0e-6d9c-4bb2-b196-b1c827a13566))
  )

  (symbol (lib_id "power:+5V") (at 29.21 39.37 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid e7348afc-e716-4e41-b502-473762a765d1)
    (property "Reference" "#PWR0102" (id 0) (at 29.21 43.18 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Value" "+5V" (id 1) (at 29.21 34.29 0))
    (property "Footprint" "" (id 2) (at 29.21 39.37 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 29.21 39.37 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 71148a58-c6a4-4ca7-87d1-da4204cea5b2))
  )

  (symbol (lib_id "Interface_CAN_LIN:TJA1051T") (at 222.25 107.95 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid e85479a1-246b-4094-ab2f-e2441217b8b6)
    (property "Reference" "U2" (id 0) (at 224.2694 95.25 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TJA1051T" (id 1) (at 224.2694 97.79 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-223-8" (id 2) (at 222.25 120.65 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://www.nxp.com/documents/data_sheet/TJA1051.pdf" (id 3) (at 222.25 107.95 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid ba12b919-266b-49e0-8c9a-cd852982ad76))
    (pin "2" (uuid 6a31060f-6af7-4ff7-881b-4bd0403498b4))
    (pin "3" (uuid 63d57e58-1d9b-44cb-8e5e-34d48fa96f84))
    (pin "4" (uuid b53297b9-b708-4ab8-87e2-5856dafbf067))
    (pin "5" (uuid e2802236-0b9d-4378-acc3-ff56c139e92e))
    (pin "6" (uuid 92259475-6959-4be9-99fb-5b87a080c7dc))
    (pin "7" (uuid dc6cb566-6bf9-4b64-8af9-7dc0b2417d25))
    (pin "8" (uuid ef77e506-7008-4d46-8706-e95f795db707))
  )

  (symbol (lib_id "Device:C") (at 114.3 140.97 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid ec78bac1-6c96-46f4-8243-b3ab845fedef)
    (property "Reference" "C1" (id 0) (at 118.11 139.6999 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "14 pF" (id 1) (at 118.11 142.2399 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "" (id 2) (at 113.3348 137.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 114.3 140.97 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 4be067af-8718-431d-8d75-106f087c2b06))
    (pin "2" (uuid 2753d1eb-fab9-48d1-97f5-4c7e27359263))
  )

  (sheet_instances
    (path "/" (page "1"))
  )

  (symbol_instances
    (path "/6117d579-0678-4c3b-8682-2fe4ddc7a0e7"
      (reference "#PWR0101") (unit 1) (value "GNDREF") (footprint "")
    )
    (path "/e7348afc-e716-4e41-b502-473762a765d1"
      (reference "#PWR0102") (unit 1) (value "+5V") (footprint "")
    )
    (path "/ec78bac1-6c96-46f4-8243-b3ab845fedef"
      (reference "C1") (unit 1) (value "14 pF") (footprint "digikey-footprints:0603")
    )
    (path "/68e9e548-d824-4d92-b10b-c055a20dcada"
      (reference "C2") (unit 1) (value "14 pF") (footprint "digikey-footprints:0603")
    )
    (path "/36540234-f263-4775-a9eb-82bf31b6d3b0"
      (reference "C3") (unit 1) (value "100 nF") (footprint "digikey-footprints:0603")
    )
    (path "/2c236797-4e84-4743-80c6-9d38d6188d4c"
      (reference "J1") (unit 1) (value "Conn_01x04_Female") (footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-4-3.5-H_1x04_P3.50mm_Horizontal")
    )
    (path "/6b0bd125-8e7d-4e87-97f5-0d4d53faa173"
      (reference "J2") (unit 1) (value "Conn_01x08_Female") (footprint "Connector_PinHeader_1.00mm:PinHeader_1x08_P1.00mm_Vertical_SMD_Pin1Left")
    )
    (path "/0ddffb29-819f-4fb1-8ac1-f59fa3272ba3"
      (reference "JP1") (unit 1) (value "Jumper_2_Open") (footprint "Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Vertical_SMD_Pin1Right")
    )
    (path "/76ee4584-81e2-4930-acce-1ecd238cf151"
      (reference "R1") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path "/58697035-c2a5-4a72-aa6c-0845690bbd5f"
      (reference "R2") (unit 1) (value "120") (footprint "digikey-footprints:0603")
    )
    (path "/55870dc1-a751-4fb1-a7eb-fe844b64659b"
      (reference "U1") (unit 1) (value "MCP2515-xSO") (footprint "Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm")
    )
    (path "/e85479a1-246b-4094-ab2f-e2441217b8b6"
      (reference "U2") (unit 1) (value "TJA1051T") (footprint "Package_TO_SOT_SMD:SOT-223-8")
    )
    (path "/70b5de83-b371-4d8a-b6ce-c6eae87736b1"
      (reference "U3") (unit 1) (value "MCP1703A-5002_SOT23") (footprint "Package_TO_SOT_SMD:SOT-23")
    )
    (path "/7308e13a-4809-4e8e-af65-9905819aa376"
      (reference "U4") (unit 1) (value "ATmega4809-A") (footprint "Package_QFP:TQFP-48_7x7mm_P0.5mm")
    )
    (path "/a9ccf595-ea22-4b8c-914d-3ab6dbf2ada1"
      (reference "Y1") (unit 1) (value "16 MHz") (footprint "Crystal:Crystal_SMD_SeikoEpson_MC156-4Pin_7.1x2.5mm_HandSoldering")
    )
  )
)
